{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["Instructions","Pattern Creator","Reference Images","Box Presets"],"not_rendered":{"charts":0,"images":7,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Instructions","index":0,"n_rows":46,"n_cols":6,"rows_kept":46,"cut":false,"hidden":false,"merged":[[39,2,39,15],[33,2,33,15],[41,1,42,15],[28,2,30,15],[27,2,27,15],[31,2,31,15],[15,2,17,14],[20,2,24,15],[25,2,25,15],[19,2,19,15],[34,2,38,15]]}
[]
[]
[null,"Welcome to the H.B. Fuller FullCheck™ Stencil Service Pattern Creator!"]
[]
[null,"Objective:"]
[null,"This tool is used to replicate the adhesive pattern on an end-of-line packaging application for a product SKU."]
[null,"Using this information FullCheck tools can be created to ensure you are not only putting the correct amount of adhesive on, but also in the correct areas. "]
[null,"A completed Pattern Creator file must be uploaded at the point of purchase for each pattern/SKU desired."]
[]
[null,"Need help completing the FullCheck™ Pattern Creator?                      to request FullVision™ Pro and let our experts build the ideal stencil for your packaging line!"]
[]
[null,"Instructions"]
[]
[null,"Get Started by clicking ",null,null,null,"on the Pattern Creator sheet"]
[]
[null,null,"First, you need to select a box type from the available options.  A reference image will appear in the side panel as you select an option to compare to your box, but please note that these images are generic representations of the specified box type.\nAfter selecting appropriate box type, click \"Confirm Dimensions\" to proceed."]
[]
[]
[]
[null,null,"Next, you will need to dimension the flaps that see adhesive, whether through direct application or after folding and compression."]
[null,null,"a)  First, select the unit you will be dimensioning in.\nb)  Then, either select an individual flap or check the box indicating that multiple flaps have identical dimensions.  The flap(s) you are currently dimensioning will be highlighted on the reference image in the side panel.\nc)  Next, input the flap length and width (as defined on the form) into the appropriate fields.  Click       for more detailed instructions when completing this form.\nd) Finally, Click \"Save Dimensions\" to store the inputs."]
[]
[]
[]
[]
[null,null,"Once all flaps have been either dimensioned or deemed as \"Not Applicable\", click \"Confirm Dimensions\" to continue."]
[]
[null,null,"The last form to complete allows you to specify a bead tolerance for your pattern and desired settings for the application."]
[null,null,"a) Select the length and width tolerances, which defines the margin (±) around the target bead location.\nb) Use the check boxes to select/deselect the criteria that is shown on the adhesive stencil.  Once a box is checked, you can input the appropriate settings and unit (if applicable).  Units can be toggled through by clicking the appropriate toggle button.  Click       for more detailed instructions when completing this form."]
[]
[]
[null,null,"After selecting the bead tolerances and any desired application settings, click \"Create Pattern\" to begin adding beads to your substrate."]
[]
[null,null,"Finally, you will need to add the adhesive pattern to your substrate and upload reference pictures (optional)."]
[null,null,"a) Add beads to any flap by simply clicking on the flap in the reference box, which will pull up the dimensioned flap and bead addition form.  Define the bead position and length parameters, using the checkboxes indicating parallel, identical beads and/or stitched beads, as needed.  The beads will display on the reference box after you click \"Add Beads\".  Additional beads can be added to a flap, or entirely deleted from a flap, using the bead addition form after clicking a flap in the reference box.\nNote: You only need to add beads to one flap, not both that eventually come together under compression.\nb) Individual beads can be edited or deleted by clicking on them in the dimensioned flap, and the stencil specifications can be changed and/or added to by clicking"]
[]
[]
[]
[]
[null,null,"c) Reference pictures (max of 9) can be added to help describe your pattern by clicking"]
[]
[null,"Once all beads have been added to your pattern, and all references images you would like to add have been imported, click                                   and email the completed file to FullVision@hbfuller.com"]
[]
[]
[]
[null,"© 2018 H.B. Fuller Company"]

{"sheet":"Pattern Creator","index":1,"n_rows":35,"n_cols":7,"rows_kept":35,"cut":false,"hidden":false,"merged":[[1,1,18,5],[19,1,19,5],[21,1,21,5],[10,6,11,6]]}
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Bead flap scale = 1:1"]
[]
[]
[null,null,null,null,null,null,"Red dot indicates the flap's top, left corner"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"reference image not to scale",null,null,null,null,"© 2018 H.B. Fuller Company"]
[]
[null,"        Application Specifications"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,266.30526733398437]
[null,null,null,null,null,null,39.872676849365234]

{"sheet":"Reference Images","index":2,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
[]
[null,"Click on an image to remove it"]

{"sheet":"Box Presets","index":3,"n_rows":28,"n_cols":13,"rows_kept":28,"cut":false,"hidden":true,"merged":[[0,0,0,4]]}
["When adding boxes, update the loop in SaveStencil() and AdjustSpec()",null,null,null,null,null,null,null,"Pressure","Nozzle","Tank","Hose","Gun"]
["Index","BoxTypes","Flaps","Flap Nomenclature (24 character limit)","Code",null,null,null,"psi","in","°F Tank","°F Hose","°F Gun"]
[0,"*** Cases ***",null,null,"#NA",null,"Object","Name","Text"]
[1,"Regular Slotted Case (RSC)",8,"Major, Top, Mach; Minor, Trailing, Mach; Minor, Leading, Mach; Major, Bottom, Mach; Major, Top, Op; Minor, Trailing, Op; Minor, Leading, Op; Major, Bottom, Op","RSC",null,"flap","RSC:Major, Top, Mach","position",null,"Total\nLength",{"$f":"IF($L$6=\"in\", M4/72, M4/28.35)","v":4.5},324]
[2,"Half Slotted Case (HSC)",4,"Major, Top, Mach; Minor, Trailing, Mach; Minor, Leading, Mach; Major, Bottom, Mach","HSC",null,"flap bead","Major, Top, Mach:01.01","BoxType",null,"TotalTol",{"$f":"IF($L$6=\"in\", M5/72, M5/28.35)","v":0.75},54]
[3,"Wrap-Around RSC",9,"Major, Top, Mach; Minor, Trailing, Mach; Minor, Leading, Mach; Major, Bottom, Mach; Major, Top, Op; Minor, Trailing, Op; Minor, Leading, Op; Major, Bottom, Op; Manufacturer's Joint","RWA",null,"sample flap","RSC_Major, Top, Mach","Vr_Hr",null,null,"in","points"]
[4,"Wrap-Around HSC",5,"Major, Top, Mach; Minor, Trailing, Mach; Minor, Leading, Mach; Major, Bottom, Mach; Manufacturer's Joint","HWA",null,"sample bead","Major, Top, Mach_01.01","(none)",null,"Lt",0.125]
[5,"Tray",6,"Tab, Trailing, Mach; Flap, Trailing; Tab, Trailing, Op; Tab, Leading, Mach; Flap, Leading; Tab, Leading, Op","TRE",null,"tolerance\nbox","Major, Top, Mach-01.01","Lt_Wt (current)",null,"Wt",0.125]
[6,"Bag-In-Box (1 piece)",9,"Major, Top, Mach; Minor, Trailing, Mach; Minor, Leading, Mach; Major, Bottom, Mach; Major, Top, Op; Minor, Trailing, Op; Minor, Leading, Op; Major, Bottom, Op; Manufacturer's Joint","BIB"]
[7,"*** Cartons ***",null,null,"#NA"]
[8,"Dry Goods Carton",9,"Major, Top, Mach; Minor, Trailing, Mach; Minor, Leading, Mach; Major, Bottom, Mach; Major, Top, Op; Minor, Trailing, Op; Minor, Leading, Op; Major, Bottom, Op; Manufacturer's Joint","DGC"]
[9,"Beverage Carton (12pk cans)",8,"Major, Top, Mach; Minor, Trailing, Mach; Minor, Leading, Mach; Major, Bottom, Mach; Major, Top, Op; Minor, Trailing, Op; Minor, Leading, Op; Major, Bottom, Op","BVC"]
[]
[null,null,null,null,null,"Ideas"]
[null,null,null,null,null,"General Ideas:","Different beads have different colors (order of checking?)"]
[null,null,null,null,null,"SaveStencil():","Copy all flaps/sample box to a new sheet?"]
[null,null,null,null,null,"Dimension_Flaps:","Auto-fill dimensions for common box types (i.e. 12pk cans)"]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,"Statements & Assumptions"]
[null,null,null,null,null,"All beads on a flap are either horizontal or vertical, not a mix of both"]
[null,null,null,null,null,"Beads added at different times don't \"see\" each other (allows for overlap)"]
[null,null,null,null,null,"All flaps are rectangular"]
[null,null,null,null,null,"Bead widths are always 5 points"]